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NEGATIVE PRESSURE UNIT AIR-PRO/10000H


 NEGATIVE PRESSURE UNIT AIR-PRO/10000H

DESCRIPTION:
	Negative Pressure Unit, designed to maintain negative pressure in asbestos removal activities. 
	The housing, front panel, and rear cover are made of powder-coated aluminum, making the unit lightweight and durable. It is specially designed for long-term use and for ease of handling.
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FEATURES:
- Nominal airflow capacity of 10000 m3/h 
- Variable flow control
- Automatic soft start
- HEPA filter H14: 99.995% filtration
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El contenido generado por IA puede ser incorrecto.]- Dimensions (LxWxH): 1030x690x1165 mm
	- Weight: 92 kg
	- Power supply: 230 Volt, 50 Hz
	- Operating current: 13 A
	- Motor power: 3 kW
	- Exhale hose connection: Ø545 mm
	- 2-step filter system: 
	     Pre-filter EU4: 610x910x94 mm
	     HEPA filter acc. to EN 1822 Class H14: 915x610x292 mm
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