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NEGATIVE PRESSURE UNIT AIR-PRO/3000H


 NEGATIVE PRESSURE UNIT AIR-PRO/3000H

DESCRIPTION:
	Negative Pressure Unit, designed to maintain negative pressure in asbestos removal activities. 
	The housing, front panel, and rear cover are made of powder-coated aluminum, making the unit lightweight and durable. It is specially designed for long-term use and for ease of handling.
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FEATURES: 
- Nominal airflow capacity of 3000 m3/h 
- Variable flow control
- Automatic soft start
- HEPA filter H14: 99.995% filtration
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[bookmark: _Hlk214262454][image: ]- Dimensions (LxWxH): 945x420x850 mm
	- Weight: 39 kg
	- Power supply: 230 Volt, 50 Hz
	- Operating current: 3,3 A
	- Motor power: 0,75 kW
	- Exhale hose connection: Ø295 mm
	- 2-step filter system: 
	     Pre-filter EU4: 289x595x94 mm
	     HEPA filter acc. to EN 1822 Class H14: 305x610x292 mm
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